|  | Tutorial - Modeling a Spas 12 |  |
|  | Right, time to make the handle. Roughly extrude the box you just created to flow along the handle, something along the line of this: Now select all the very our vertices and scale them in [using shift :)] and scale them in Using the same process do the name to the next layer this'll get you a curve, not which vertices I've scaled in and which I have ignored, hide any vertices that get in the way. I found my handle wasn't curvy, so I made the inner parts wider, you may need to do the same. Now, this requires you own skill, you'll need to align the vertices to the handle's shape, keeping the thinner ones at the edge of the handle, and the middle set in between the inner and outer set, I'm afraid its hard to get right, even I can struggle, but keep at it, time and patience is the key. Handle done, now for the trigger guard. Create a four sectioned extruded box - Move them to fit them to the image Now in bottom view, with back faces ignored select the bottom faces of the extruded box. Now, extrude it downwards, while moving at rotating, then scale and move any vertices that are out of shape, by now you should be able to manage it :) Click 'Next to continue' <<< Back | Next>>> |  |
|  | Site © Matthew McDonald 2003 |  |