|  | Tutorial - Modeling a Spas 12 |  |
|  | Now hide it all and save quickly. Generate a cylinder and turn it to face you. (don't know why I didn't hide it) Select the inner faces by using the face selection tool and selecting the middle vertex (Cylinder move so you can see) Now slam extrude again and scale it inwards... ...then click extrude again and in the front view move it across so the front lines up with the back. then delete the back vertices and align the back of what now is a 'tube'. You've made a tube :D, but please don't celebrate just yet, we've got to put it into position. Firstly align the middle vertices with the angled ones to make a straight edge on either side, use the vertex align stuff again. Extend the top to stretch it, guessed where we're putting it yet? Rotate it to that bit sticking out on the stock and resize if necessary. Now for the detailing of it. align the vertices to that of the hinge we created like this: (not far to go - by now I'm ready to Murder frontpage - keeps adjusting fonts!) Now scale and position the tube on the front view - must poke out both sides (Selected one is the tube) Click 'Next to continue' <<< Back | Next>>> |  |
|  | Site © Matthew McDonald 2003 |  |