|  | Tutorial - Modeling a Spas 12 |  |
|  | Great not far off, I'm now onto the 100th image, happy tutorial picture, a whole century of pics :P Just joking, back to serious work. Grab you new flat group and extrude it outwards to get it 3d. Now, duplicate what is selected and drag it over to the other side of the object and duplicate - don't regroup it just yet. because you've aligned it, you've lost the selection, so go into the groups tab and reselect the group (be sure to de-select anything first). Now reverse vertex order, (Ctrl+Shift+F or Alt+C+Enter). Now you can regroup :) Duplicate the new group and go into Vertex > Mirror Left<-->Right' in the top toolbar. It should duplicate the shell ladder like this: Next, select all the faces except the end ones as if you wished to extrude them: (don't extrude though) Then, hide the faces to leave you with this in the front view: Then, select these faces and extrude them along the shape of the stock into 3 sections. Now align the end vertices into the curved cylinder shape at the end. Now unhide everything and put the two sides of the ladder to each end of the main gun, so its all in line. Now for the base of the shell ladder, simply create a box, very easy and scale and move into position. Easy as pie :) (easiest bit in the world) Now Just dump in a cylinder at the hinge of the stock (by god this is easy, wont stay easy for too long) Click 'Next to continue' <<< Back | Next>>> |  |
|  | Site © Matthew McDonald 2003 |  |